# 2026-03-10 22:40:31 by RouterOS 7.19.2
# software id = CIAZ-SUFT
#
# model = RB5009UG+S+
# serial number = HEE08K82CQV
/interface bridge
add name=local port-cost-mode=short
/interface wireless security-profiles
set [ find default=yes ] supplicant-identity=MikroTik
/ip pool
add name=dhcp_pool0 ranges=192.168.88.2-192.168.88.254
add name=dhcp_pool1 ranges=192.168.88.10-192.168.88.254
/ip dhcp-server
add address-pool=dhcp_pool1 interface=local lease-time=10m name=dhcp2
/ip smb users
add name=cjones
add name=chris
/ip smb
set enabled=yes
/interface bridge port
add bridge=local interface=ether2 internal-path-cost=10 path-cost=10
add bridge=local interface=ether3 internal-path-cost=10 path-cost=10
add bridge=local interface=ether4 internal-path-cost=10 path-cost=10
add bridge=local interface=ether5 internal-path-cost=10 path-cost=10
add bridge=local interface=ether6 internal-path-cost=10 path-cost=10
add bridge=local interface=ether7 internal-path-cost=10 path-cost=10
add bridge=local interface=ether8 internal-path-cost=10 path-cost=10
add bridge=local interface=ether1 internal-path-cost=10 path-cost=10
/ip firewall connection tracking
set udp-timeout=10s
/interface ovpn-server server
add mac-address=FE:73:F4:5A:2B:60 name=ovpn-server1
/ip address
add address=192.168.88.1/24 interface=local network=192.168.88.0
/ip dhcp-client
add interface=sfp-sfpplus1
/ip dhcp-server lease
add address=192.168.88.239 client-id=1:0:11:32:28:2:98 mac-address=\
    00:11:32:28:02:98 server=dhcp2
add address=192.168.88.47 client-id=1:48:a9:8a:c0:95:a mac-address=\
    48:A9:8A:C0:95:0A server=dhcp2
add address=192.168.88.232 client-id=1:dc:a6:32:67:1:16 mac-address=\
    DC:A6:32:67:01:16 server=dhcp2
add address=192.168.88.231 client-id=1:a8:a1:59:ae:a0:3e mac-address=\
    A8:A1:59:AE:A0:3E server=dhcp2
add address=192.168.88.15 client-id=1:dc:cd:2f:b:aa:b1 mac-address=\
    DC:CD:2F:0B:AA:B1 server=dhcp2
add address=192.168.88.87 client-id=1:5c:f9:dd:e5:41:eb mac-address=\
    5C:F9:DD:E5:41:EB server=dhcp2
add address=192.168.88.26 client-id=1:c8:b2:9b:db:b0:23 mac-address=\
    C8:B2:9B:DB:B0:23 server=dhcp2
add address=192.168.88.250 client-id=1:e0:2b:e9:cf:dc:d5 mac-address=\
    E0:2B:E9:CF:DC:D5 server=dhcp2
add address=192.168.88.20 client-id=1:dc:21:5c:84:3a:a5 mac-address=\
    DC:21:5C:84:3A:A5 server=dhcp2
add address=192.168.88.144 comment="Static IP for Clinitek engine" \
    mac-address=3E:BE:90:50:0E:47
add address=192.168.88.138 client-id=\
    ff:f8:ce:1b:a1:0:2:0:0:ab:11:6f:15:1:e4:34:20:3c:8c mac-address=\
    A2:53:3A:64:F4:DE server=dhcp2
add address=192.168.88.25 client-id=1:bc:f8:7e:8f:32:ea mac-address=\
    BC:F8:7E:8F:32:EA server=dhcp2
add address=192.168.88.40 client-id=\
    ff:e4:96:b0:28:0:2:0:0:ab:11:a:d3:57:3f:cd:69:67:6c mac-address=\
    DC:A6:32:67:01:17 server=dhcp2
/ip dhcp-server network
add
add address=192.168.88.0/24 dns-server=192.168.88.231,192.168.88.40 gateway=\
    192.168.88.1 wins-server=0.0.0.0
/ip dns
set allow-remote-requests=yes servers=8.8.8.8
/ip firewall filter
add action=accept chain=input comment="accept established,related" \
    connection-state=established,related
add action=drop chain=input connection-state=invalid
add action=accept chain=input comment="allow ICMP" in-interface=sfp-sfpplus1 \
    protocol=icmp
add action=accept chain=input comment="allow Winbox" in-interface=\
    sfp-sfpplus1 port=8291 protocol=tcp
add action=accept chain=input comment="allow SSH" in-interface=sfp-sfpplus1 \
    port=22 protocol=tcp
add action=drop chain=input comment="block everything else" in-interface=\
    sfp-sfpplus1
/ip firewall nat
add action=masquerade chain=srcnat out-interface=sfp-sfpplus1
add action=dst-nat chain=dstnat dst-address=173.48.126.187 dst-port=80 \
    protocol=tcp to-addresses=192.168.88.231 to-ports=80
add action=dst-nat chain=dstnat dst-address=173.48.126.187 dst-port=8080 \
    protocol=tcp to-addresses=192.168.88.231 to-ports=8080
add action=dst-nat chain=dstnat dst-address=173.48.126.187 dst-port=443 \
    protocol=tcp to-addresses=192.168.88.231 to-ports=443
add action=dst-nat chain=dstnat dst-address=173.48.126.187 dst-port=8070 \
    protocol=tcp to-addresses=192.168.88.231 to-ports=8070
add action=dst-nat chain=dstnat dst-address=173.48.126.187 dst-port=52199 \
    protocol=tcp to-addresses=192.168.88.231 to-ports=52199
add action=dst-nat chain=dstnat dst-address=173.48.126.187 dst-port=3389 \
    protocol=tcp to-addresses=192.168.88.250 to-ports=3389
add action=dst-nat chain=dstnat dst-address=173.48.126.187 dst-port=443 \
    protocol=tcp to-addresses=192.168.88.231 to-ports=443
/ip ipsec profile
set [ find default=yes ] dpd-interval=2m dpd-maximum-failures=5
/ip smb shares
set [ find default=yes ] directory=/pub disabled=no
add directory=demoshare name=demoshare
/system clock
set time-zone-name=America/New_York
/system identity
set name=RB5009
